#
SLIDING DOOR CIRCUIT CONTACT REMOVAL/INSTALLATION

BME0911739A0W01

## Door Side

1. Disconnect the negative battery cable.

2. Remove the sliding door trim.

3. Disconnect the sliding door circuit contact connector.

4. Remove the bolts.

5. Remove the sliding door circuit contact.

6. Install in the reverse order of removal.

## Body Side

1. Disconnect the negative battery cable.

2. Remove the B-pillar lower trim.

3. Disconnect the sliding door circuit contact connector.

4. Remove the bolts.

5. Remove the sliding door circuit contact.

6. Install in the reverse order of removal.