#
NO.26 HOLD INDICATOR LIGHT DOES NOT ILLUMINATE WHEN HOLD SWITCH IS TURNED TO ON [JA5A-EL]

BME050301030262

26 | HOLD indicator light does not illuminate when HOLD switch is turned to ON
DESCRIPTION | • HOLD indicator light in instrument cluster does not illuminate when the HOLD switch is turned on with the ignition switch at ON.
POSSIBLE CAUSE | • HOLD switch or related wiring harness malfunction.

  Note

  • Before following the troubleshooting steps, make sure that the Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Do other indicator lights illuminate with the ignition switch at on? | Yes | Go to the next step.
No | Inspect the meter fuse.
2 | Inspect the TCS PID value using the WDS or equivalent. Is the TCS PID value normal? | Yes | Go to the next step.
No | Inspect the HOLD switch. (See HOLD SWITCH INSPECTION [JA5A-EL].) If the HOLD switch normal, inspect for continuity between the HOLD switch and TCM terminal 2I.
3 | Remove the HOLD indicator light. Is the HOLD indicator light bulb burned out? | Yes | Replace the HOLD indicator light.
No | Inspect for open circuit or disconnected connector in following harness. • Ignition switch and HOLD indicator light • HOLD indicator light and TCM terminal E including instrument cluster circuit board
4 | • Verify the test results.

  - If normal, return to the diagnostic index to service any additional symptoms.
  - If the malfunction remains, inspect the related Service Bulletins and/or On-line Repair Information and perform repair or diagnosis.

  • If the vehicle is repaired, troubleshooting is completed.
  • If the vehicle is not repaired or additional diagnostic information is not available, replace the TCM.