#
TRANSAXLE CONTROL MODULE (TCM) DESCRIPTION [JA5A-EL]

BME051718901T02

## Outline

• The TCM controls the automatic transaxle operations. The TCM outputs a control signal to the transaxle according to the signal from other sensors and/or switches.
• In driving mode, there are three mode selections: NORMAL, high temp, and SLOPE. The TCM automatically selects the proper mode according to driving condition.