#
CONNECTORS

A6E201700006E02

## Data link connector

• Insert the probe into the terminal when connecting a jumper wire to the data link connector.

  Caution

  • Inserting a jumper wire probe into the data link connector terminal may damage the terminal.

## Disconnecting connectors

• When disconnecting connector, grasp the connectors, not the wires.

• Connectors can be disconnected by pressing or pulling the lock lever as shown.

## Locking connector

• When locking connectors, listen for a click indicating they are securely locked.

## Inspection

• When a tester is used to inspect for continuity or measuring voltage, insert the tester probe from the wiring harness side.

• Inspect the terminals of waterproof connectors from the connector side since they cannot be accessed from the wiring harness side.

  Caution

  • To prevent damage to the terminal, wrap a thin wire around the tester probe before inserting into terminal.

## Terminals

### Inspection

  • Pull lightly on individual wires to verify that they are secured in the terminal.

## Wiring Harness

### Wiring color codes

  • Two-color wires are indicated by a two-color code symbol.
  • The first letter indicates the base color of the wire and the second the color of the stripe.

CODE | COLOR | CODE | COLOR
--- | --- | --- | ---
B | Black | O | Orange
BR | Brown | P | Pink
G | Green | R | Red
GY | Gray | V | Violet
L | Blue | W | White
LB | Light Blue | Y | Yellow
LG | Light Green |  |