#
WHEEL HUB, HUB SPINDLE REMOVAL/INSTALLATION

BME031205000W03

  Caution

  • Performing the following procedures without first removing the ABS wheel-speed sensor may possibly cause an open circuit in the harness if it is pulled by mistake. Before performing the following procedures, remove the ABS wheel-speed sensor (axle side) and fix it to an appropriate place where the sensor will not be pulled by mistake while the vehicle is being serviced.

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

1 | Hub cap
2 | Locknut (See Locknut Removal Note) (See Locknut Installation Note)
3 | Brake drum
4 | Wheel hub and ABS sensor rotor
5 | ABS sensor rotor (See ABS Sensor Rotor Removal Note) (See ABS Sensor Rotor Installation Note)
6 | Hub bolt (See Hub Bolt Removal Note) (See Hub Bolt Installation Note)
7 | Wheel hub
8 | Parking brake cable
9 | Brake pipe
10 | Rear brake component
11 | Hub spindle

## Locknut Removal Note

1. Raise the staked portion of the locknut using a small cape chisel and a hammer.

2. Lock the hub by applying the brakes.

3. Remove the locknut.

## ABS Sensor Rotor Removal Note

  Note

  • The sensor rotor does not need to be removed unless it is being replaced.

1. Remove the sensor rotor using a chisel.

## ABS Sensor Rotor Installation Note

  Caution

  • Position the SST so that marking B faces the bottom.

1. Set the SST as shown in the figure.

2. Press on the new sensor rotor using the SST and a press.

## Locknut Installation Note

1. Install a new locknut and stake it as shown.