#
DRIVE BELT CONSTRUCTION [AJ]

BME011015800T03

## Front Drive Belt

• A single V-ribbed belt (serpentine type) has been adopted on the front drive belt which drives the generator, P/S oil pump and the A/C compressor. A drive belt auto tensioner inside the coil spring has been adopted which is automatically adjusted so that the appropriate tension from the tensioner pulley is maintained.
• The front drive belt tension is automatically adjusted so that appropriate tension from the auto tensioner for the front drive belt is maintained.

1 | P/S pump pulley
2 | Generator pulley
3 | Front drive belt
4 | A/C compressor pulley
5 | Drive belt auto tensioner
6 | Crankshaft pulley