#
LIFTGATE LOCK ACTUATOR INSPECTION

BME091462310201

1. Remove the liftgate lower trim.

2. Disconnect the liftgate lock actuator connector.

3. Apply battery positive voltage to the liftgate lock actuator terminals and inspect the operation of the liftgate lock actuator.

  • If not as specified, replace the liftgate lock.

Connection | Actuator operation
--- | ---
B+ | GND
B | A | Lock
A | B | Unlock