#
NO.28 HOLD INDICATOR LIGHT ILLUMINATE WHEN HOLD SWITCH IS NOT TURNED TO ON [FN4A-EL]

BME050301030232

28 | HOLD indicator light illuminate when HOLD switch is not turned to ON
DESCRIPTION | • HOLD indicator light in instrument cluster illuminate even though the HOLD switch is turned off with the ignition switch at ON.
POSSIBLE CAUSE | • HOLD switch or related wiring harness malfunction.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Inspect the HOLD switch. (See HOLD SWITCH INSPECTION [FN4A-EL].) Is the HOLD switch normal? | Yes | Go to the next step.
No | Repair or replace any malfunctioning parts.
2 | Disconnect the PCM connector. Turn the ignition switch off. Is the resistance between 3Q terminal at the PCM connector and the body ground more than 10 kilohms? | Yes | Replace the PCM.
No | Repair short circuit between the HOLD indicator light and PCM. Reconnect the PCM.