#
CYLINDER HEAD (II) DISASSEMBLY

A6E242402000E06

1. Disassemble in the order indicated in the table.

1 | Engine hanger
2 | Valve keeper (See Valve Keeper Disassembly Note)
3 | Upper valve spring seat
4 | Valve spring
5 | Valve
6 | Valve seal (See Valve Seal Disassembly Note)
7 | EGR pipe
8 | Water outlet case

## Valve Keeper Disassembly Note

1. Remove the valve keeper using the SSTs.

## Valve Seal Disassembly Note

1. Remove the valve seal using the SST.