#
POWER STEERING OIL PUMP (AJ) REMOVAL/INSTALLATION

BME061232650202

1. Remove in the order indicated in the table.

2. Remove the No.3 engine joint bracket. (See ENGINE REMOVAL/INSTALLATION [AJ].)

3. Install in the reverse order of removal.

4. Adjust the No.3 joint bracket. (See ENGINE REMOVAL/INSTALLATION [AJ].)

1 | Drive belt
2 | Power steering oil pump pulley
3 | Pressure switch connector
4 | Pressure pipe
5 | Return hose
6 | Power steering oil pump cover
7 | Power steering oil pump