#
AFTER REPAIR PROCEDURE [MZR-CD (RF Turbo)]

BME011400000W07

  Warning

  • Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injuries or death and damage. When installing the fuel hose, observe "Fuel Hose Installation" described below.

## Fuel Line Air Bleeding

  Caution

  • Continuously cranking the engine for over 30 seconds can damage the battery and the starter.

1. Continue cranking the engine for 30 seconds and stop for 5-10 seconds until the engine starts.

## Fuel Hose Installation

1. Verify that there is no damage or deformation on the fuel hose and fuel pipe when installing.