#
PANEL LIGHT CONTROL SWITCH REMOVAL/INSTALLATION

BME091866600201

1. Disconnect the negative battery cable.

2. Remove the driver-side side panel.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

1 | Panel light control switch (See Panel Light Control Switch Removal Note.)
2 | Connector

## Panel Light Control Switch Removal Note

1. Insert your hand into the hole in the driver-side side panel, squeeze the tabs of the panel light control switch and pull it forward to remove.