#
REAR POWER WINDOW REGULATOR REMOVAL/INSTALLATION

BME091272560W01

1. Disconnect the negative battery cable.

2. Remove the rear door glass. (See SLIDING DOOR DISASSEMBLY/ASSEMBLY.)

3. Disconnect the rear power window regulator connector.

4. Remove the nuts and the rear power window regulator.

Tightening torque

  6.87-9.80 N·m {70-100 kgf·cm, 60.8-86.7 in·lbf}

5. Install in the reverse order of removal.