#
DOOR SWITCH REMOVAL/INSTALLATION

BME091866540201

## Front

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Screw
2 | Connector
3 | Door switch

## Rear

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Bolt
2 | Connector
3 | Door switch