#
NO.24 ENGINE STALLS WHEN SHIFTED TO D, S, L RANGES, OR IN R POSITION [FN4A-EL]

BME050301030228

24 | Engine stalls when shifted to D, S, L ranges, or in R position
DESCRIPTION | • Engine stalls when shifting from N or P position to D, S, L ranges or R position at idle.
POSSIBLE CAUSE | • The malfunction is on the engine control side (i.e. IAC system). Otherwise, the malfunction is in the input/turbine speed sensor (engine sometimes starts) or the TCC circuit (engine always stalls).

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Go to No.10 "LOW IDLE/STALLS DURING DECELERATION". (See NO.10 LOW IDLE/STALLS DURING DECELERATION [L3].) Is the engine control system normal? | Yes | Repeat the basic inspection and repair or replace any malfunctioning parts according to the inspection result. (See BASIC INSPECTION [FN4A-EL].)
No | Repair or replace any malfunctioning parts according to the inspection results.