#
UPPER MODULE REMOVAL/INSTALLATION

BME092066900203

1. Disconnect the negative battery cable.

2. Remove the audio unit.

3. Remove in the order indicated in the table.

1 | Screw (See Screw Installation Note.)
2 | Upper module (See Upper Module Removal Note.)
3 | Cover (See Cover Removal Note.)

4. Install in the reverse order of removal.

## Upper Module Removal Note

1. Insert a screwdriver into the hole stamped mark.

2. To remove upper module, lift it by pushing down the screwdriver's handle.

## Cover Removal Note

1. Insert a tape-wrapped screwdriver between the cover and the base unit, then unlatch hook A.

2. To unlatch hook B, pull the cover upward.

## Screw Installation Note

  Caution

  • If an undesignated screw is used, the inside of the upper module could be damaged. When installing the module, be sure to use a designated screw (red).