#
SLIDING DOOR CIRCUIT CONTACT REMOVAL/INSTALLATION

BME091100104201

  Warning

  • Handling the side air bag sensor improperly can accidentally deploy the side air bag module, which may seriously injure you. Read AIR BAG SYSTEM SERVICE WARNINGS before working around the B-pillar areas. (See SERVICE WARNINGS.)

  Note

  • The side air bag sensor is located in the B-pillar.

## Door Side

1. Disconnect the negative battery cable.

2. Remove the sliding door trim. (See SLIDING DOOR TRIM REMOVAL/INSTALLATION.)

3. Disconnect the sliding door circuit contact connector.

4. Remove the bolts.

5. Remove the sliding door circuit contact.

6. Install in the reverse order of removal.

## Body Side

1. Disconnect the negative battery cable.

2. Remove the B-pillar lower trim.

3. Disconnect the sliding door circuit contact connector.

4. Remove the bolts.

5. Remove the sliding door circuit contact.

6. Install in the reverse order of removal.