#
SHIFT MECHANISM REMOVAL/INSTALLATION [G15M-R]

BME051646010W02

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

3. After installation, verify that the gear shift lever operates smoothly when the clutch pedal is depressed.

.

1 | Shift lever knob
2 | Cover
3 | Console (See REAR CONSOLE REMOVAL/INSTALLATION.)
4 | Boot
5 | Transverse member
6 | Bolt
7 | Nut
8 | Bushing
9 | Nut
10 | Washer
11 | Shift lever component