#
CRANKSHAFT POSITION (CKP) SENSOR REMOVAL/INSTALLATION [L3]

BME014018220W02

## Removal

1. Perform the following procedure to making the working space.

  (1) Remove the Front wheel (RH).
  (2) Remove the splash shield.

2. Disconnect the CKP sensor connector.

3. Remove the installation bolts to remove the CKP sensor.

## Installation

  Caution

  • When foreign material, such as an iron chips, gets on the CKP sensor, it can cause abnormal output from the sensor because of flux turbulence and adversely affect engine control. Be sure there is no foreign material on the CKP sensor when replacing.

1. Perform the following procedure so that piston No.1 is at the top dead center.

  (1) Remove the driveshaft (RH). (See DRIVE SHAFT REMOVAL/INSTALLATION [L3].)
  (2) Remove the cylinder block lower blind plug and install the SST.
  (3) Turn the crankshaft pulley to the clockwise until it stops.

2. Using a straight edge, draw a straight line directly in the center of the ninth tooth of the crankshaft pulley pulse wheel (counting counterclockwise from the empty space).

  Caution

  • If the line is not accurately drawn, ignition timing, fuel injection and other engine control systems will be adversely effected. Drawn the straight line carefully using a straight edge.

3. Align the center line of the crankshaft position sensor and the line drawn in Step 2, then install the sensor.

4. Install the CKP sensor fitting bolts.

Tightening torque

  5.5-7.5 N·m {56-76 kgf·cm, 4.1-5.5 ft·lbf}

5. Remove the SST then install the cylinder block lower blind plug.

Tightening torque

  20 N·m {2.0 kgf·m, 15 ft·lbf}

6. Install the front driveshaft (RH). (See DRIVE SHAFT REMOVAL/INSTALLATION [L3].)