#
INTERIOR LIGHT REMOVAL/INSTALLATION

BME091851311W01

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Interior light
2 | Connector
3 | Lens (See Lens Removal Note.)
4 | Interior light bulb

## Lens Removal Note

1. Insert a tape-wrapped flathead screwdriver into the service hole.

2. Push the tabs to remove the lens.