#
HEADLIGHT BULB REMOVAL/INSTALLATION

BME091851030201

  Caution

  • A halogen bulb generates extremely high heat when it is used. If the surface of the bulb is soiled, excessive heat will build up and the light's life will be shortened. When replacing the bulb, hold the metal flange, not the glass.

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Connector
2 | Cover (See Cover Installation Note)
3 | Headlight bulb (See Headlight Bulb Removal Note)

3. Install in the reverse order of removal.

## Headlight Bulb Removal Note

1. Release the bulb seating wire to remove the headlight bulb.

## Cover Installation Note

1. Install the cover with the 'TOP' mark facing up.