#
INTERMITTENT CONCERN TROUBLESHOOTING [MZR-CD (RF Turbo)]

BME010300103269

## Vibration Method

1. If a malfunction occurs or becomes worse while driving on a rough road, or due to engine vibration, perform the steps below.

  Note

  • There are several reasons that the vehicle or engine vibration could cause an electrical malfunction. Some of the things to inspect for are:

  - Connectors not fully seated.
  - Wiring harnesses not having full play
  - Wiring harnesses laying across brackets or moving parts
  - Wiring harnesses routed too close to hot parts

  • An improperly routed, improperly clamped, or loose wiring harness can cause wiring harness to become pinched between parts.
  • The connector joints, points of vibration, and places where the wiring harnesses pass through the fire wall, body panels, etc. are the major areas to be checked.

## Inspection Method for Switch Connectors or Wiring harnesses

1. Connect the WDS or equivalent to the DLC-2.

2. Turn the engine switch to the ON position (Engine off).

  Note

  • If the engine starts and runs, perform the following steps at idle.

3. Access PIDs for the switch you are inspecting.

4. Turn the switch on manually.

5. Shake each connector or wiring harness a bit vertically and horizontally while monitoring the PID.

  • If the PID value is unstable, check for poor connection.

## Inspection Method for Sensor Connectors or Wiring harnesses

1. Connect the WDS or equivalent to the DLC-2.

2. Turn the engine switch to the ON position (Engine off).

  Note

  • If engine starts and runs, perform the following steps at idle.

3. Access PIDs for the switch you are inspecting.

4. Shake each connector or wiring harness a bit vertically and horizontally while monitoring the PID.

  • If the PID value is unstable, check for poor connection.

## Inspection Method for Sensors

1. Connect the WDS or equivalent to the DLC-2.

2. Turn the engine switch to the ON position (Engine off).

  Note

  • If the engine starts and runs, perform the following steps at idle.

3. Access PIDs for the switch you are inspecting.

4. Vibrate the sensor slightly with your finger.

  • If the PID value is unstable or a malfunction occurs, check for poor connection and/or poorly mounted sensor.

## Inspection Method for Actuators or Relays

1. Connect the WDS or equivalent to the DLC-2.

2. Turn the engine switch to the ON position (Engine off).

  Note

  • If the engine starts and runs, perform the following steps at idle.

3. Prepare the Output State Control for actuators or relays that you are inspecting.

4. Vibrate the actuator or relay with your finger for 3 s after Output State Control is activated.

  • If a variable click sound is heard, check for poor connection and/or poorly mounted actuator or relay.

  Note

  • Vibrating relays too strongly may result in open relays.

## Water Sprinkling Method

  Caution

  • Indirectly change the temperature and humidity by spraying water onto the front of the radiator.
  • If a vehicle is subject to water leakage, the leakage may damage the control module. When testing a vehicle with a water leakage problem, special caution must be used.

If a malfunction occurs only during high humidity or rainy/snowy weather, perform the following steps.

1. Connect the WDS or equivalent to the DLC-2 if you are inspecting sensors or switches.

2. Turn the engine switch to the ON (Engine off).

  Note

  • If the engine starts and runs, perform the following steps at idle.

3. Access PIDs for sensor or switch if you are inspecting sensors or switches.

4. If you are inspecting a switch, turn it on manually.

5. Spray water onto the vehicle or run it through a car wash.

  • If the PID value is unstable or a malfunction occurs, repair or replace the part if necessary.