#
NO.2 VEHICLE MOVES IN N POSITION [FN4A-EL]

BME050301030206

2 | Vehicle moves in N position
DESCRIPTION | • Vehicle creeps in N position. • Vehicle creeps if brake pedal is not depressed in N position.
POSSIBLE CAUSE | • If the vehicle moves in N position, basically, the malfunction is in the ATX. Since a malfunction in the sensor circuit or output circuit is the cause of the malfunction in the ATX, inspect the sensors, output circuit, and the related wiring harnesses.

  1. Clutch burnt (Forward clutch)

  • Control valve body malfunction

  2. Selector lever position disparity (Although the selector indicator shows N position, hydraulic circuit shows D range or R position)

  Note

  • Before following the troubleshooting steps, make sure that the Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Does the vehicle creep when the selector lever is moved slightly in N position? | Yes | Go to the next step.
No | Adjust the selector lever. (See SELECTOR CABLE ADJUSTMENT.)
2 | Disconnect the PCM connector. Is the resistance between the ground terminal at the PCM connector and the body ground less than 5.0 ohms? | Yes | Go to the next step.
No | Repair open ground circuit. Reconnect the PCM.
3 | Inspect the LPS PID value using the WDS or equivalent. Is the LPS PID value normal? (See PCM INSPECTION [L3].) | Yes | Overhaul the control valve body and repair or replace any malfunctioning parts. (See ATX workshop manual (FN4A-EL).) If any problem remains, overhaul the transaxle and repair or replace any malfunctioning parts. (See ATX workshop manual (FN4A-EL).)
No | Repair or replace any malfunctioning parts.