#
REAR ANTENNA FEEDER No.2 REMOVAL/INSTALLATION

BME092066942W03

1. Disconnect the negative battery cable.

2. Remove the liftgate upper trim.

3. Remove the headliner.(See HEADLINER REMOVAL/INSTALLATION.)

4. Disconnect the connection between the rear antenna feeder No.1 and the rear antenna feeder No.2.

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

1 | Bolt
2 | Rear antenna feeder No.2