#
CENTER PILLAR INSTALLATION

BME098070350B02

1. After installing and trial-fitting the inner, the reinforcement, and the side sill reinforcement, plug weld during installation of the outer.

2. When joining the new and old parts, temporarily install and fit the new part in position, measure each dimension according to the body dimension drawing, then adjust the position to align it to the standard dimension.

3. After trial-fitting new parts, make sure the related parts fit properly.