#
COWL GRILLE REMOVAL/INSTALLATION

BME091650790W01

1. Remove the windshield wiper arm and blade. (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Weatherstrip
2 | Cover
3 | Screw
4 | Cowl grille (See Cowl Grille Installation Note.)

## Cowl Grille Installation Note

1. Verify that the clip installation holes on the cowl grille are not deformed.

2. If deformed, repair them using a plastic hammer, then install the cowl grille.