#
REAR PILLAR (OUTER) AND CORNER PLATE INSTALLATION

BME098070442B02

1. When joining the new and old parts, temporarily install and fit the new part in position, measure each dimension according to the body dimension drawing, then adjust the position to align it to the standard dimension.

2. After trial-fitting new parts, make sure the related parts (Liftgate, Rear combination light) fit properly.

3. Welding of (F) should be performed during installation of the rear end panel.

4. Welding of (G) should be performed during installation of the rear fender panel.