#
NO.25 A/C IS NOT CUT OFF UNDER WIDE OPEN THROTTLE CONDITIONS [L3]

BME010300000W27

25 | A/C IS NOT CUT OFF UNDER WOT CONDITIONS.
--- | ---
DESCRIPTION | A/C compressor magnetic clutch does not disengage under WOT.
POSSIBLE CAUSE | • TP sensor malfunction • TP sensor misadjustment • Loosely installed TP sensor.

Diagnostic procedure

STEP | INSPECTION | RESULTS | ACTION
--- | --- | --- | ---
1 | Does A/C compressor disengage when A/C switch is turned off? | Yes | Go to next step.
No | Go to symptom troubleshooting "No.24 A/C is always on or A/C compressor runs continuously".
2 | Connect WDS or equivalent to DLC-2. Retrieve any continuous memory, KOEO and KOER DTCs. Are there any DTCs displayed? | Yes | DTC is displayed: Go to appropriate DTC test.
No | No DTC is displayed: Inspect TP sensor for proper adjustment.
3 | Verify test results. • If okay, return to diagnostic index to service any additional symptoms. • If malfunction remains, replace PCM.