#
AUTOMATIC TRANSAXLE LOCATION INDEX [FN4A-EL]

BME051701074201

1 | ATF (See MECHANICAL SYSTEM TEST [FN4A-EL]) (See ROAD TEST [FN4A-EL])
2 | HOLD switch (See HOLD SWITCH INSPECTION [FN4A-EL])
3 | Transaxle range (TR) switch (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [FN4A-EL]) (See TRANSAXLE RANGE (TR) SWITCH REMOVAL/INSTALLATION [FN4A-EL]) (See TRANSAXLE RANGE (TR) SWITCH ADJUSTMENT [FN4A-EL])
4 | Transaxle fluid temperature (TFT) sensor (See TRANSAXLE FLUID TEMPERATURE (TFT) SENSOR INSPECTION [FN4A-EL]) (See TRANSAXLE FLUID TEMPERATURE (TFT) SENSOR REMOVAL/INSTALLATION [FN4A-EL])
5 | Oil pressure switch (See OIL PRESSURE SWITCH INSPECTION [FN4A-EL]) (See OIL PRESSURE SWITCH REMOVAL/INSTALLATION [FN4A-EL])
6 | Input/turbine speed sensor (See INPUT/TURBINE SPEED SENSOR INSPECTION [FN4A-EL]) (See INPUT/TURBINE SPEED SENSOR REMOVAL/INSTALLATION [FN4A-EL])
7 | VSS (See VEHICLE SPEED SENSOR (VSS) INSPECTION [FN4A-EL]) (See VEHICLE SPEED SENSOR (VSS) REMOVAL/INSTALLATION [FN4A-EL])
8 | Solenoid valve (See SOLENOID VALVE INSPECTION [FN4A-EL]) (See SOLENOID VALVE REMOVAL/INSTALLATION [FN4A-EL])
9 | HOLD indicator light (See HOLD INDICATOR LIGHT INSPECTION [FN4A-EL])
10 | PCM (See PCM INSPECTION [FN4A-EL]) (See PCM REMOVAL/INSTALLATION [FN4A-EL])
11 | Automatic transaxle (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [FN4A-EL])
12 | Oil seal (See OIL SEAL REPLACEMENT [FN4A-EL])
13 | Control valve body (See CONTROL VALVE BODY REMOVAL [FN4A-EL]) (See CONTROL VALVE BODY INSTALLATION [FN4A-EL])
14 | Oil cooler (See OIL COOLER FLUSHING [FN4A-EL]) (See OIL COOLER REMOVAL/INSTALLATION [FN4A-EL])
15 | Drive plate (See DRIVE PLATE REMOVAL/INSTALLATION [FN4A-EL])