#
ON-BOARD DIAGNOSTIC SYSTEM ACTIVE COMMAND MODES FUNCTION

BME040267650T04

Active Command Modes Table

Command Name | Definition | Operation | Note
--- | --- | --- | ---
PMP_MOTOR | ABS motor | ON/OFF | Ignition key at ON (engine OFF), and driving
RF_OUTLET | Right front ABS pressure reduction solenoid valve | ON/OFF
RF_INLET | Right front ABS pressure retention solenoid valve | ON/OFF
LF_OUTLET | Left front ABS pressure reduction solenoid valve | ON/OFF
LF_INLET | Left front ABS pressure retention solenoid valve | ON/OFF
RR_OUTLET | Right rear ABS pressure reduction solenoid valve | ON/OFF
RR_INLET | Right rear ABS pressure retention solenoid valve | ON/OFF
LR_OUTLET | Left rear ABS pressure reduction solenoid valve | ON/OFF
LR_INLET | Left rear ABS pressure retention solenoid valve | ON/OFF
ABSVLVRLY | Fail-safe relay | ON/OFF
CHK_TRAC* | Check traction control indicator | ON/OFF
TRAC_OFF* | Traction control off indicator | ON/OFF
ENG_TQR* | Engine torque reduction signal output | Nm
VS_OUTPUT | Vehicle speed signal | KPH/MPH

  * :
With TCS

  Note

  • When operating the ABS motor and each valve using the active command mode, turn ABSVLVRLY ON, and then each command ON. ABSVLVRLY regulates the power supply for the ABS motor and all eight valves.