#
NO.1 MELTING OF MAIN OR OTHER FUSES [AJ]

BME010300103206

1 | Melting of main or other fuses
[TROUBLESHOOTING HINTS] Inspect condition of fuse.

Damaged Fuse | Related Wiring Harness
--- | ---
MAIN | MAIN fuse • IG KEY2 fuse • BTN fuse | • FAN1 fuse • FAN2 fuse
IG KEY1 | IG KEY1 fuse • Ignition switch

  - ENGINE fuse

FUEL PUMP | FUEL PUMP fuse • Fuel pump relay

  - Fuel pump unit

BTN | BTN fuse • ROOM fuse |
IG KEY2 | IG KEY2 fuse • Ignition switch |
FAN1 | FAN1 fuse • Cooling fan relay

  - Fan control module

FAN2 | FAN2 fuse • Cooling fan relay

  - Fan control module

ROOM | ROOM fuse • Immobilizer unit | • DLC-2
ENGINE | ENGINE fuse • Main relay • Capacitor | • Ignition coils • HO2S
EGI INJ | EGI INJ fuse • Main relay

  - EGR valve
  - EGR boost sensor solenoid valve*
  - Purge solenoid valve
  - MAF sensor
  - Fuel injectors
  - IMCC actuator
  - Fuel pump relay

• EEC fuse
• PCM
EEC | EEC fuse • PCM |

  * :
Used for Australian, General (L.H.D. R.H.D.) specs.

If malfunction remains, refer to related Service Information and perform repair or diagnosis.

• If vehicle is repaired, troubleshooting completed.
• If vehicle is not repaired or additional diagnostic information is not available, replace or reprogram the PCM.