#
REAR WIPER MOTOR INSPECTION

BME091967450202

1. Disconnect the negative battery cable.

2. Remove the liftgate lower trim.

3. Disconnect the rear wiper motor connector.

4. Connect battery positive voltage to the rear wiper motor terminal A and the ground to a bare metal part of the vehicle and the rear wiper motor terminal B.

5. Verify that the rear wiper motor operates.

6. Disconnect the ground to the terminal B while the rear wiper is operating.

7. Verify that the rear wiper stops in the park position.

  • If not as specified, replace the rear wiper motor.