#
SLIDING DOOR TRIM REMOVAL/INSTALLATION

BME091768520W01

1. Disconnect the negative battery cable if equipped with power window systm.

2. Remove the sliding door garnish.

3. Remove the sliding door inner handle.

4. Remove the regulator handle if equipped.

5. Disengage clips A using a fastener remover.

6. Pull the sliding door trim upward, then disengage hook B from the body.

7. Disconnect the power window subswitch connector if equipped.

8. Remove the sliding door trim.

9. Install in the reverse order of removal.