#
BODY & ACCESSORIES NEW FEATURES

BME090000000T05

## Improved safety

• Automatic window return function has been added for driver-side power window system. (Australian, European (L.H.D. U.K.) specs.)
• Shock absorbing parts have been adopted for occupant head protection.

## Improved convenience

• The rear doors are of sliding design.
• The open lock has been adopted for the sliding door.
• An answer back function has been adopted for the keyless entry system. (Except vehicles with theft-deterrent system)
• The IG OFF timer function and the two-step down function have been adopted for the power window system.
• A side table has been adopted for the passenger-side front seat.
• Assist grips have been adopted for the front seat backs.
• A sliding mechanism has been adopted for the second-row seats.
• A side-sliding mechanism has been adopted for the second-row seat.
• A third-row seat that can be stowed has been adopted.

## Improved visibility

• The heated outside mirrors have been added. (European (L.H.D. U.K.), General (L.H.D.) specs.)

## Improved marketability

• The second- and third-row seats have been made removable.
• A warning light and indicator lights have been added in instrument cluster.
• The theft-deterrent system has changed with the addition of the answer-back function to the keyless entry system.
• A car-navigation system has been newly added.
• A 2-DIN size audio unit has been adopted. It provides various, extendable combinations (CD player/CD changer/cassette deck/MD player).

## Improved comfort

• Seat warmer system has been adopted for the front seats. (European (L.H.D.) specs.)

## Improved quietness

• The bracket mounted to the windshield wiper motor absorbs the vibration due to motor operation and reduces variation in wipe angle.

## Improved serviceability

• DTCs 01, 07, 17, 20, and 42 of the input/output check mode in the instrument cluster have been added.
• A diagnostic assist function has been adopted to the audio unit.

## Improved design

• Two types front bumpers are available: standard and sports.
• The rear bumper with protectors has been adopted.
• A power sliding door (PSD) system, which allows the sliding doors to open/close automatically, has been adopted for both LH and RH sliding doors.
• A front combination light with built-in front turn and parking light has been adopted.
• Two types front fog lights are available: standard and sports.
• A front flap has been adopted.

## Improved security

• Double locking system has been added to power door lock system. (European (L.H.D. U.K.) specs.)