#
KEYLESS UNIT REMOVAL/INSTALLATION

BME091401097W01

## L.H.D.

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Keyless unit connector
2 | Nut
3 | Keyless unit

3. Install in the reverse order of removal.

## R.H.D.

1. Disconnect the negative battery cable.

2. Remove the glove compartment.

3. Disconnect the short cord and vehicle side harness connector.

4. Remove the nut, then remove the keyless unit.

5. Install in the reverse order of removal.