#
NO.10 FREQUENT SHIFTING [JA5A-EL]

BME050301030246

10 | Frequent shifting
DESCRIPTION | • Downshifting occurs suddenly even when accelerator pedal is depressed slightly in D, S, L ranges except HOLD mode.
POSSIBLE CAUSE | • The malfunctioning circuit is basically the same as No.9 "ABNORMAL SHIFTING". However, a malfunction of the input signal to the TP sensor, input/turbine speed sensor, VSS (including the sensor GND, sensor wiring harness and connector), or clutch slippage (clutch stuck, low pressure in line) may also be the cause.

  Note

  • Before following the troubleshooting steps, make sure that the Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.