#
REAR HEATER CORE REMOVAL/INSTALLATION

BME071161410W01

1. Disconnect the negative battery cable.

2. Drain the engine coolant.(See ENGINE COOLANT REPLACEMENT [L3].) (See ENGINE COOLANT REPLACEMENT [MZR-CD (RF Turbo)].)

3. Remove the right side trunk side trim.

4. Remove the rear heat duct No.4.

5. Remove as indicated in the table.

6. Install in the reverse order of removal.

1 | Rear heater hose No.1 (See Heater Pipe and Hose Component Installation Note)
2 | Rear heater hose No.2 (See Heater Pipe and Hose Component Installation Note)
3 | Rear heater core