#
INTERMITTENT REAR WIPER RELAY REMOVAL/INSTALLATION

BME091966810201

  Note

  • Because the lock section of the relay is damaged easily, do not remove it from the bracket unless replacement is necessary. Always perform an inspection of the intermittent wiper relay before removal.

1. Disconnect the negative battery cable.

2. Remove the bracket.

3. Disconnect the connector.

4. Remove the intermittent rear wiper relay.

5. Install in the reverse order of removal.