#
FRONT DOOR REMOVAL/INSTALLATION

BME091158010W01

1. Disconnect the negative battery cable.

2. To remove the front door hinge, remove the front fender panel.

3. Remove the front door trim.

4. To remove the checker, remove the door speaker.

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

7. Adjust the front door. (See FRONT DOOR ADJUSTMENT.)

1 | Connector (See Connector Removal Note.) (See Connector Installation Note.)
2 | Front door hinge
3 | Front door
4 | Checker

## Connector Removal Note

1. Push the rubber boot backward.

2. Pull the pin up.

## Connector Installation Note

1. Connect the connector and the rubber boot.

2. Push the pin down.

3. Install the rubber boot on the body.