#
GUIDE BLADE ACTUATOR INSPECTION [MZR-CD (RF Turbo)]

BME011313700W02

1. Disconnect the vacuum hose from the guide blade actuator.

2. Connect the vacuum pump to the guide blade actuator.

3. Apply vacuum and verify that the rod moves as specified.

Specification

Vacuum (kPa {mmHg, inHg}) | Rod movement
--- | ---
Below -14.5 {-108, -4.27} | Starts to move
Above -44.9 {-337, -13.3} | Fully pulled

  • If not as specified, replace the turbocharger.