#
CAR-NAVIGATION UNIT CONSTRUCTION

BME092066902T01

## Terminal Layout and Signals

Terminal | Signals
--- | ---
24-pin connector
| 1A | Left front speaker (+)
1B | B+ (power back up)
1C | Left front speaker (-)
1D | Right front speaker (+)
1E | Illumination (+)
1F | Right front speaker (-)
1G | Illumination (-)
1H | Ant. Cont.
1I | Vehicle speed
1J | Amp. Cont.
1K | Parking brake switch
1L | -
1M | R range
1N | Steering SW1
1O | -
1P | Steering SW2
1Q | -
1R | ACC
1S | Left rear speaker (+)
1T | -
1U | Left rear speaker (-)
1V | Right rear speaker (+)
1W | Ground
1X | Right rear speaker (-)

Terminal | Signals
--- | ---
13-pin connector
| 1 | Ground
2 | B+ (power back up)
3 | Left input (+)
4 | -
5 | -
6 | Bus (+)
7 | Right input (+)
8 | Right input (-)
9 | ACC
10 | Bus (-)
11 | Left input (-)
12 | Illumination
13 | -