#
HEADLIGHT CLEANER SWITCH REMOVAL/INSTALLATION

BME091951030207

1. Disconnect the negative battery cable.

2. Remove the driver-side side panel.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

1 | Headlight Cleaner switch (See Headlight Cleaner Switch Removal Note.)
2 | Connector

## Headlight Cleaner Switch Removal Note

1. Insert your hand into the hole for the driver-side side panel, squeeze the tabs of the headlight cleaner switch and pull it forward to remove it.