#
FRONT BUMPER REMOVAL/INSTALLATION

BME091050031201

1. Disconnect the negative battery cable.

2. Remove the front combination light. (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

3. Disconnect the front fog light connector.

4. Remove in the order indicated in the table.

Standard

Sports

1 | Bolt A
2 | Fastener
3 | Screw
4 | Bolt B
5 | Fastener
6 | Bolt C
7 | Clip
8 | Front bumper (See Front Bumper Removal Note.) (See Front Bumper Installation Note.)

5. Install in the reverse order of removal.

## Front Bumper Removal Note

1. Pull the front bumper ends (wheel arch) outward to disengage from the bumper slider.

  Caution

  • If only one side of the front bumper is disengaged from the bumper slider and the bumper falls, it could be damaged. When disengaging the front bumper from the slider, secure the bumper so that it does not fall.

2. Remove the front bumper from the body.

## Front Bumper Installation Note

1. Spread the front bumper ends (wheel arches) apart.

2. Attach the front bumper to the body.

3. Press the front bumper connections into the body to engage with the bumper slider.