#
CONTROLLER AREA NETWORK (CAN) OPERATION [AJ]

BME014000000T81
• PCM communicates with TCM through CAN as shown below.
Input

  - Reduce torque signal
  - Turbine speed signal
  - ATF temperature signal
  - Racing select determination
  - MIL indicate request signal
  - Range signal
  - TCC signal

Output

  - Engine speed signal
  - TP signal
  - Engine torque signal (without torque down)
  - Engine torque signal (with torque down)
  - Engine torque signal (torque loss)
  - Torque reduced signal
  - Battery reconnection signal
  - ECT signal