#
NO.4 EXCESSIVE CREEP [JA5A-EL]

BME050301030240

4 | Excessive creep
DESCRIPTION | • Vehicle accelerates in D, S, L ranges and R position when accelerator pedal is not depressed.
POSSIBLE CAUSE | 1. Engine idle speed is high (transaxle system is not cause of problem) 2. Go to No.9 "FAST IDLE/RUNS ON" (See NO.9 FAST IDLE/RUNS ON [AJ].)

  Note

  • Before following the troubleshooting steps, make sure that the Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.