#
DTC P0032 [L3]

BME010201084202

DTC P0032 | Front HO2S heater circuit high input
--- | ---
DETECTION CONDITION | • The PCM monitors the front HO2S heater control signal at PCM terminal 4A. If the PCM turns the front HO2S heater on but the front HO2S heater circuit has high voltage, the PCM determines that the front HO2S heater circuit has malfunction.

  Note

  • The front HO2S heater is controlled by a duty signal.

Diagnostic support note
• This is an intermittent monitor (O2 sensor heater).
• MIL illuminates if PCM detects the above malfunction condition in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the PCM.
• PENDING CODE is available if PCM detects the above malfunction condition.
• FREEZE FRAME DATA is available.
• DTC is stored in PCM memory.
POSSIBLE CAUSE | • Short to power circuit between front HO2S terminal D and PCM terminal 4A • Front HO2S or PCM terminal is shorted • Front HO2S heater malfunction • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | PERFORM DTC CONFIRMATION PROCEDURE • Perform DTC CONFIRMATION PROCEDURE. (See DTC CONFIRMATION PROCEDURE [L3].) • Is the same DTC present? | Yes | Go to the next step.
No | Intermittent concern exists. Go to INTERMITTENT CONCERN TROUBLESHOOTING procedure. (See INTERMITTENT CONCERN TROUBLESHOOTING [L3].)
2 | INSPECT FRONT HO2S TERMINALS • Turn the ignition switch off. • Disconnect the front HO2S connector. • Inspect for bent terminals. • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 6.
No | Go to the next step.
3 | INSPECT FRONT HO2S HEATER • Inspect the front HO2S heater. (See HEATED OXYGEN SENSOR (HO2S) INSPECTION [L3].) • Is the front HO2S heater normal? | Yes | Go to the next step.
No | Replace the front HO2S, then go to Step 6.
4 | INSPECT PCM TERMINAL • Disconnect the PCM connector. • Inspect for bent terminals. • Is there any malfunction? | Yes | Repair the terminal, then go to Step 6.
No | Go to the next step.
5 | INSPECT FRONT HO2S HEATER CONTROL CIRCUIT FOR SHORT TO POWER CIRCUIT • Turn the ignition switch to the ON position (Engine off). • Measure the voltage between front HO2S terminal D (wiring harness-side) and body ground. • Is the voltage B+? | Yes | Repair or replace the wiring harness for shot to power circuit, then go to the next step.
No | Go to the next step.
6 | VERIFY TROUBLESHOOTING OF DTC P0032 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Perform KOEO/KOER self-test. (See KOEO/KOER SELF-TEST PROCEDURE [L3].)
• Is the same DTC present?
Yes
Replace the PCM, then go to the next step.
(See PCM REMOVAL/INSTALLATION [L3].)
No | Go to the next step.
7 | VERIFY AFTER REPAIR PROCEDURE • Perform "After Repair Procedure". (See AFTER REPAIR PROCEDURE [L3].) • Is there any DTC present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [L3].)
No | Troubleshooting completed.