#
REAR WIPER MOTOR REMOVAL/INSTALLATION

BME091967450W01

1. Disconnect the negative battery cable.

2. Remove the rear wiper arm and blade. (See REAR WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

3. Remove the liftgate lower trim.

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

6. Adjust the rear wiper arm and blade. (See REAR WIPER ARM AND BLADE ADJUSTMENT.)

1 | Connector
2 | Outer bushing
3 | Bolt
4 | Rear wiper motor