#
POWER SLIDING DOOR (PSD) SYSTEM OUTLINE

BME091173001101

• The sliding doors open/close automatically by the following switches and buttons:

Switch and button | Sliding door position
--- | ---
Fully closed | Partly open | Fully open
PSD front OPEN switch | Open | Open | Not operation
PSD front CLOSE switch | Not operation | Close | Close
PSD rear switch | Open | Open | Close
Transmitter R or L button | Open | Open | Close

• When any of the following switches or buttons are pressed while the door is sliding, the door is stopped. (To stop a door, a switch or a button for the corresponding door should be pressed.)

  - PSD front OPEN/CLOSE switch
  - PSD rear switch
  - Transmitter R or L button

• When opening/closing a sliding door using the inner or outer handle, the sliding door slides automatically in the operating direction via the handle assist function.

• Using the main switch, operation of the sliding doors can be switched between power and manual sliding.

• When each switch or button is operated, the buzzer sounds for 0.5 second to indicate that a sliding door is starting to open/close.

• When a sliding door contacts an obstruction during opening/closing operation, the door reverses direction automatically to prevent jamming.

• During closing, when the sliding door reaches a point approximately 200 mm {7.87 in} before full closure, closing speed slows for safety.

• The PSD system is controlled by the PSD control module.

• The sliding door is slid by the PSD drive module.

• The easy closure system assists the sliding door to close fully when it is ajar.

• The sliding door latch is released by the latch release actuator.