#
THIRD-ROW SEAT OPERATION

BME091357200T02

## Stowing Third-row Seat Operation

1. Remove the headrests.

2. Pull strap A and fold the seat back forward.

3. Pull strap B while lifting the seat up and to the rear.

1 | Third-row seat
2 | Strap A
3 | Strap B

## Rear View Seating Operation

1. Open the liftgate.

2. Remove the headrests.

3. Pull strap B while supporting the seat back with the other hand and carefully ease the seat back rearward and into the seat well.

4. Set the hook on the seat back support bar in the rear of the seat back.

5. Pull the seat back towards the front of the vehicle until the opposite end of the support bar hooks onto the anchor loop.

1 | Front
2 | Rear
3 | Strap B
4 | Seat back support bar
5 | Hook
6 | Anchor loop