#
FRONT FOG LIGHT BULB REMOVAL/INSTALLATION

BME091851680201

  Caution

  • A halogen bulb generates extremely high heat when it is used. If the surface of the bulb is soiled, excessive heat will build up and the light's life will be shortened. When replacing the bulb, hold the metal flange, not the glass.

1. Disconnect the negative battery cable.

2. Remove the mud guard.

3. Remove in the order indicated in the table.

Standard

Sports

1 | Connector
2 | Spring (Standard)
3 | Front fog light bulb (See Front Fog Light Bulb Removal Note)

4. Install in the reverse order of removal.

## Front Fog Light Bulb Removal Note

1. Turn the front fog light bulb to the arrow mark and remove it.